Highlights

* A method to estimate crystal filterability based on a specified CSD is proposed.
* Simulation results are validated using published experimental data.
* A case study of an ammonium alum production process is provided.
* A tradeoff between crystallizer and filter design is analyzed quantitatively.
* Source code is publically available on Github.